Each audio file contains the vowel sounds generated with one particular resonator for all five pressure values in a sequence (0.8, 1.0, 1.2, 1.4, 1.6 kPa), where the duration for each pressure value is about 1 s.
